605-100

Land Rover Supplementary Rear Lamp Wiring Guide.

We recommend connections to the vehicle wiring harness are made in the area of the rear R/H lamps, remove the internal access panel (90/110) to expose the wiring loom & connections to rear lamps.

Kit includes Twin Core extension cables, a Yellow Butt Connector to enable multiple earth connections, 10 Red Butt Connectors to connect the lamps to the provided cables and 6 Scotchloks for the +ve connections and earth connection from the Yellow Butt.

 **Lamp Lamp Wire Colour Harness Wire Colour**

L/H Indicator Brown Green/Red

 White Black

L/H Tail Lamp Brown Red/Black (Red)

 White Black

-----------------------------------------------------------------------------------------------

High Level Stop Red Green/Purple

 White Black

-----------------------------------------------------------------------------------------------

R/H Indicator Brown Green/White

 White Black

L/H Tail Lamp Brown Red/Orange (Red)

 White Black

*(Red) denotes up to and including Series 3 vehicles.*